---------------------------
----- SCAME PARRE SpA -----
-- SLActive  Application --
---------------------------

<-- ITALIAN README -->

Fare sempre riferimento ai manuali di installazione, configurazione ed uso del prodotto prima di utilizzare gli applicativi sotto descritti.

PROCEDURA DI INSTALLAZIONE:
1 - estrarre il contenuto dell'intero archivio
2 - installare i driver del programmatore, contenuti in "\Driver_ProgrammatoreActive" (nome eseguibile "CP210xVCPInstaller.exe")
3 - Eseguire uno dei programmi SLActive presenti, seguento le modalità a seguito

SLActive_v1.3.exe
Permette la programmazione delle tessere MiFare in caso di Hardware basato su MAX1 e MAX2

SLActive_admin_v2.0.exe
Permette la programmazione delle tessere MiFare in caso di versione EVSE Firmware installata inferiore a 1.3.044.2 (la versione è visibile all'avvio della stazione di ricarica)

SLActive_admin_v2.1.exe
Permette la programmazione delle tessere MiFare in caso di versione Firmware installata uguale o successiva a 1.3.044.2 (la versione è visibile all'avvio della stazione di ricarica)

SLSetup_v1.0.exe
Permette di impostare i parametri specifici delle elettroniche MAX1 e MAX2


<-- ENGLISH README -->

Please always refer to installation, configuration and use manuals before using any of the programs described below.

HOW TO INSTALL:
1 - extract all the .zip content
2 - install the driver in "\Driver_ProgrammatoreActive" (.exe name "CP210xVCPInstaller.exe")
3 - execute one of SLActive applications, according to what written below

SLActive_v1.3.exe
This program allows the programming of MiFare cards in case of MAX1 and MAX2 electronics based EVSE 

SLActive_v2.0_admin.exe
This program allows the programming of MiFare cards if the Firmware version of the station onboard electronics is minor to 1.3.044.2 (the version is visible during the boot process)

SLActive_v2.1_admin.exe
This program allows the programming of MiFare cards if the Firmware version of the station onboard electronics is equal or major to 1.3.044.2 (the version is visible during the boot process)

SLSetup_v1.0.exe
This program allows the user to set some specific parameters on MAX1 and MAX2 based electronics