Instructions for installation of card programmer


1. Install driver "CP210xVCPInstaller.exe"
2. Connect the programmer on USB port
3. From "Device Manager" in "System Properties" check the COM port number
   assigned to device "CP210x"
4. Run "SLActive.exe"
5. In "options" select COM port assigned

Further information on "USER MANUAL - CHARGING STATIONS FOR ELECTRIC VEHICLES"
